New C5b collimator with integrated ion getter pump

At z = −1.45 m: ’GG Transition’

• Design finished mid Feb 2003.

• Procurement of parts and manufacturing on critical path through AV and ZM, completed by mid May ’03.

• Assembly by H1. 4 day bakeout at 148^oC.

• Final pressure and spectrum accepted by MVA on 2.6.03.

• IGP tested in the old ZEUS compensator magnet.

Good pumping in the range 10^{−5} down to 5 · 10^{−8} mbar, limited by outgassing from test setup.

Vacuum Review D. Pitzl, 13.6.2003

Tasks

• GG transition nstalled yesterday.

• Connection of water cooling and temperature sensors in progress.

• Vacuum system ±26 m connected.

Pump down over weekend, Leak search on Monday.

Vacuum Review D. Pitzl, 13.6.2003