Short Guide To The FPS Control PC

Are pots IN or OUT?

Look at yellow Way field for each station: Way ≈ 0: Pots are OUT

≈ stable at 25..48mm (90V, 81V): vert. stations IN ≈ stable at 20..26mm (80H, 64H): hor. stations IN

To Move The Pots IN With Automatics

1. lumi declared and FPS HV set to Full HV ?!? 2. red rightmost rate changing, > 0 and < 10kHz ?!? 3. HERA, HERA-B and ZEUS are informed ?!? 4. HERA-B is not moving wire target ?!? If yes ⇒ click blue Start button to move Pots in with the automatic procedure.

Lumi End Or Beam Loss

Retract each pot with it’s own blue RETRACT button. Failure? ⇒ red Emergency RETRACT button on the PC. Failure? ⇒ red EMERGENCY RETRACT button ABOVE the PC.

Pots Were Thrown Out By Spike??

Please turn the page!

Emergency??

Please turn the page!

Pots Were Thrown Out By Spike??

Click confirmation panel AND the green QUIT button below the red Emergency RETRACT button. If all else looks well ⇒ move pots in again.

Emergency??

1. PC running ⇒ use Emergency RETRACT button 2. PC not running or failure?

Use Red EMERGENCY RETRACT button ABOVE PC OR Red FPS OFF button in Room 301

In case of any problems or questions call the FPS Expert on call