rf-strips25 mm implant pitch50 mm readout pitchaluminium wire bondscarbon fiber railAPC128 amplifierand pipeline chipCeramic Hybrid

221 mm

34 mm

4.4mm

640 readout lineson 2nd metal layer z-strips88 mm pitch vias metal-1 to metal-2 n-side:p-side:

Decoder chip

CST Half-Ladder

Kapton cable