1 The COZ: recover from trips

T. Kurča, 12.8.1998

1. If COZ channel trips then

ffl wait at least 5 minutes

(don’t hurry - it has tripped only 1 channel, the rest of the chamber is on!)

ffl click ”ON” - to ramp up the tripped channel

2. If the same channel trips after few minutes again

ffl wait approximately 25 minutes ffl click ”ON” - to ramp up the tripped channel

3. If the same channel trips again (3rd times)

ffl don’t try to ramp it up ffl watch more closely the background rates and note them (Veto Wall counters, CIZ currents) ffl call the expert : Telephone - DESY 31-35 private 837439 Cityphone - 4688334

4. If all (or allmost all) channels are tripping, e.g. :

0-15 20-35 40-55 60-75 80-95 100-115

ffl switch ”OFF” the chamber ffl after 15 minutes put it into ”STANDBY” ffl inform the expert